{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["数据"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"数据","index":0,"n_rows":102,"n_cols":26,"rows_kept":102,"flags":["formulas_cached_only"]}
["序号","机具大类","机具小类","机具品目","分档名称","生产企业","产品名称","机具型号","产品投档技术参数","产品配置参数","证书编号","中央补贴额","自填补贴额","有效期截止日期\r\n","销售价格（元）","功率（kW）","机具类型","企业所属省份","产品状态","评阅结果","评阅意见","备注","翻倾防护装置强度检验报告编号","翻倾防护装置强度检验报告检测机构","可靠性试验报告编号","可靠性试验报告检测机构"]
[1,"耕整地机械","耕地机械","旋耕机","单轴1-1.5m旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-125","耕幅:1.25m;单轴:是 ","耕幅：125cm   重量230kg","部20170413","300元","300.00","2021-12-31","2300.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[2,"耕整地机械","耕地机械","旋耕机","单轴1-1.5m旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-140","耕幅:1.4m;单轴:是 ","耕幅140cm，重量250kg","部20171867","300元","300.00","2021-12-31","2500.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[3,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-180","耕幅:1.8m;单轴:是 ","单轴；工作幅宽 1800mm；外形尺寸（长×宽×高）：1120×1940×1060mm、耕深：120-180mm、配套动力：51.4-66.2kW、总安装刀数：48把、旋耕刀型号：IT245","冀2017T—238","900元","900.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[4,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-150","耕幅:1.5m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1000×1650×1000；作业速度范围：0.27～1.38m/s；工作幅宽：150cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：213/300r/min；刀辊最大回转半径：225mm；刀辊总安装刀数：36把；旋耕刀型号：IT225；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：29.5～44.1kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370350","900元","900.00","2026-08-31","3050.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[5,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-160","耕幅:1.6m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1000×1750×1000；作业速度范围：0.27～1.38m/s；工作幅宽：160cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：213/300r/min；刀辊最大回转半径：225mm；刀辊总安装刀数：40把；旋耕刀型号：IT225；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：36.8～51.5kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370350","900元","900.00","2026-08-31","3100.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[6,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-170","耕幅:1.7m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1000×1850×1000；作业速度范围：0.27～1.38m/s；工作幅宽：170cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：213/300r/min；刀辊最大回转半径：225mm；刀辊总安装刀数：44把；旋耕刀型号：IT225；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：44.1～73.5kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370350","900元","900.00","2026-08-31","3150.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[7,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-180","耕幅:1.8m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1000×2080×1000；作业速度范围：0.27～1.38m/s；工作幅宽：180cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：213/300r/min；刀辊最大回转半径：225mm；刀辊总安装刀数：52把；旋耕刀型号：IT225；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：44.1～73.5kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370350","900元","900.00","2026-08-31","3200.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[8,"耕整地机械","耕地机械","旋耕机","单轴1.5-2m旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-160","耕幅:1.6m;单轴:是 ","耕幅160cm，重量：260kg","部20170414","900元","900.00","2021-12-31","3600.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[9,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","北镇市兴农机械制造有限公司","旋耕机","1GQ-220","耕幅:2.2m;单轴:是 ","配套拖拉机标定功率范围：≥73.5 配套拖拉机动力输出轴转速：540、720r/min 旋耕机工作状态外形尺寸（长×宽×高）：1150×2440×1300mm 旋耕机作业速度范围：0.6～1.4m/s","辽2017120","1600元","1600.00","2021-12-31","7000.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[10,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","北镇市兴农机械制造有限公司","旋耕机","1GQ-230","耕幅:2.3m;单轴:是 ","配套拖拉机标定功率范围：≥73.5kw 配套拖拉机动力输出轴转速：540、720r/min 旋耕机工作状态外形尺寸（长×宽×高）：1150×2540×1300 旋耕机作业速度范围：0.6～1.4","辽2017120","1600元","1600.00","2021-12-31","7000.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[11,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-200","耕幅:2m;单轴:是 ","单轴；耕幅2000MM；外形尺寸(长×宽×高):1120×2120×1050MM、配套动力:66.2-73.5KW、总安装刀数:52把、旋耕刀型号:IT245","冀2017T—238","1600元","1600.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[12,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-220","耕幅:2.2m;单轴:是 ","单轴；耕幅2200MM；外形尺寸(长×宽×高):1160×2380×1220MM、耕深:120-180MM、配套动力:73.5-88.2KW、总安装刀数:60把、旋耕刀型号:IT245","冀2017T—237","1600元","1600.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[13,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-230","耕幅:2.3m;单轴:是 ","单轴；耕幅2300MM；外形尺寸(长×宽×高):1160×2580×1220MM、耕深:120-180MM、配套动力:73.5-88.2KW、总安装刀数:64把、旋耕刀型号:IT245","冀2017T—237","1600元","1600.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[14,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-240","耕幅:2.4m;单轴:是 ","单轴；耕幅2400MM；外形尺寸(长×宽×高):1150×2620×1220MM、耕深:120-180MM、配套动力:95.5-110.3KW、总安装刀数:64把、旋耕刀型号:IT245","冀2017T—236","1600元","1600.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[15,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-200","耕幅:2m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1120×2220×1120；作业速度范围：0.27～1.38m/s；工作幅宽：200cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：223/314r/min；刀辊最大回转半径：255mm；刀辊总安装刀数：56把；旋耕刀型号：IT245；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：51.5～73.5kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370349","1600元","1600.00","2026-08-31","6600.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[16,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-230","耕幅:2.3m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1120×2590×1120；作业速度范围：0.27～1.38m/s；工作幅宽：230cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：223/314r/min；刀辊最大回转半径：255mm；刀辊总安装刀数：60把；旋耕刀型号：IT245；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：58.8～88.2kW；配套拖拉机动力输出轴转速：540/760 r/min；","T202137370349","1600元","1600.00","2026-08-31","6800.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[17,"耕整地机械","耕地机械","旋耕机","单轴2-2.5m旋耕机","潍坊乐哈哈农业机械装备有限公司","旋耕机","1GQN-200","耕幅:2m;单轴:是 ","耕幅200cm，重量370kg","部20171868","1600元","1600.00","2021-12-31","7000.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[18,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","北镇市兴农机械制造有限公司","旋耕机","1GQ-260","耕幅:2.6m;单轴:是 ","配套拖拉机标定功率范围：≥88.3kw 配套拖拉机动力输出轴转速：540、720r/min 旋耕机工作状态外形尺寸（长×宽×高）：1150×2840×1300 旋耕机作业速度范围：0.6～1.4m/s","辽2017119","2200元","2200.00","2021-12-31","10000.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[19,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","北镇市兴农机械制造有限公司","旋耕机","1GQ-280","耕幅:2.8m;单轴:是 ","配套拖拉机标定功率范围：≥95.7kw 配套拖拉机动力输出轴转速：540、720r/min 旋耕机工作状态外形尺寸（长×宽×高）：1150×3040×1300mm 旋耕机作业速度范围：0.6～1.4m/s","辽2017119","2200元","2200.00","2021-12-31","10000.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[20,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","北镇市兴农机械制造有限公司","旋耕机","1GQ-300","耕幅:3m;单轴:是 ","配套拖拉机标定功率范围：≥103kw 配套拖拉机动力输出轴转速：540、720r/min 旋耕机工作状态外形尺寸（长×宽×高）：1150×3240×1300 旋耕机作业速度范围：0.6～1.4m/s","辽2017121","2200元","2200.00","2021-12-31","10000.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：产品图片：不符合填报要求。\r\n","","","","",""]
[21,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-250","耕幅:2.5m;单轴:是 ","单轴；耕幅2500MM；外形尺寸(长×宽×高):1150×2780×1350MM、耕深:120-180MM、配套动力:95.5-110.3KW、总安装刀数:68把、旋耕刀型号:IT245","冀2017T—236","2200元","2200.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求；承诺书错误\r\n","","","","",""]
[22,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-260","耕幅:2.6m;单轴:是 ","单轴；耕幅2600MM；外形尺寸(长×宽×高):1150×2880×1220MM、耕深:120-180MM、配套动力:102.9-117.6KW、总安装刀数:68把、旋耕刀型号:IT245","冀2017T—235","2200元","2200.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[23,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","馆陶县飞翔机械装备制造有限公司","旋耕机","1GQKGN-280","耕幅:2.8m;单轴:是 ","单轴；耕幅2800MM；外形尺寸(长×宽×高):1150×3050×1350MM、耕深:120-180MM、配套动力:110.2-132.4KW、总安装刀数:76把、旋耕刀型号:IT245","冀2017T—235","2200元","2200.00","2021-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[24,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","隆尧瑞泰专用设备有限公司","犁耕旋耕机","1LG-250","耕幅:2.5m;单轴:是 ","配套拖拉机标定功率：132.3-198.5        犁体幅宽：300mm             旋耕刀型号:IT245","T202013130103","2200元","2000.00","2025-09-21","21000.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[25,"耕整地机械","耕地机械","旋耕机","单轴2.5m及以上旋耕机","潍坊百励丰农业机械有限公司","旋耕机","1GKN-250","耕幅:2.5m;单轴:是 ","结构型式：框架型；整机外形尺寸（长×宽×高）mm：1120×2690×1120；作业速度范围：0.27～1.38m/s；工作幅宽：250cm；耕深：≥12cm；刀轴型式：单轴型；刀轴连接型式：花键式；传动型式：中间传动；运输方式：普通型；刀辊设计转速：315/352r/min；刀辊最大回转半径：255mm；刀辊总安装刀数：68把；旋耕刀型号：IT245；限深装置型式：限深板；镇压型式：拖板；配套拖拉机标定功率范围：73.5～110.3kW；配套拖拉机动力输出轴转速：760/850r/min；","T202137370348","2200元","2200.00","2026-08-31","7700.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[26,"耕整地机械","耕地机械","旋耕机","1.2-2m履带自走式旋耕机","广西玉林市德高机械有限公司","自走履带旋耕机","1GZL120","耕幅:1.2m;型式:履带自走式:是 ","配备12.13kW的国三标准排放柴油机，型号ZS1105DGⅢ；整机外形尺寸:2500*1350*1700；作业幅宽:1200mm；结构质量:760kg；传动方式:皮带传动；旋耕刀片总数量24把；履带参数：节距72mm，节数38节，履带宽度250mm，轨距620mm","T202045450064","7600元","7600.00","2025-07-08","35000.00","12.13","购机补贴(通用类)","广西壮族自治区","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[27,"耕整地机械","耕地机械","深松机","2-3铲凿铲式深松机","馆陶县飞翔机械装备制造有限公司","浅耕深松机","1SL-150","深松部件个数:3个;深松铲结构型式:凿铲式:是 ;铲间距:500mm","深松部件3铲;外形尺寸(长×宽×高):3400×1850×1480mm、配套动力:110.3-154.4kW、铲间距:500mm、深松深度:350-450mm、深松铲结构形式:凿式","冀2018T—166","1000元","1000.00","2022-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[28,"耕整地机械","耕地机械","深松机","2-3铲凿铲式深松机","青岛鲁耕农业机械有限公司","深松浅耕机","1LS-350","深松部件个数:3+3个;深松铲结构型式:凿铲式:是 ;铲间距:500mm","结构型式悬挂式；外形尺寸（长×宽×高）3750*2050*1850mm；翻转机构型式液压式；深松部件类型凿形深松铲；深松部件间距50cm；深松部件数量3+3；浅耕部件（犁体）类型基本（通用）型；浅耕部件（犁体）数量3+3；浅耕部件（犁体）幅宽50cm；犁铧类型可换铧尖型；犁壁类型栅条式；总工作幅宽150cm；限深轮（运输轮）类型限深运输一体轮；限深轮（运输轮）1个","T202161610020","1000元","1000.00","2026-01-14","0.00","","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：产品图片：不符合填报要求。\r\n","","","","",""]
[29,"耕整地机械","耕地机械","深松机","4-5铲凿铲式深松机","馆陶县飞翔机械装备制造有限公司","浅耕深松机","1SL-180","深松部件个数:4个;深松铲结构型式:凿铲式:是 ;铲间距:450mm","深松部件4铲;外形尺寸(长×宽×高):3850×2120×1610mm、配套功率:110.3-154.4kW、铲间距:450mm、深松深度:350-450mm、深松铲结构形式:凿式","冀2018T—167","1700元","1700.00","2022-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[30,"耕整地机械","耕地机械","深松机","4-5铲凿铲式深松机","馆陶县飞翔机械装备制造有限公司","翻转浅耕深松机","1SLF-180","深松部件个数:4个;深松铲结构型式:凿铲式:是 ;铲间距:450mm","深松部件左4右4个;外形尺寸(长×宽×高):3870×1750×1820mm、配套功率:110.3-154.4kW、铲间距:450mm、深松深度:350-450mm、深松铲结构形式:凿式","冀2018T—168","1700元","1700.00","2022-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[31,"耕整地机械","耕地机械","深松机","4-5铲凿铲式深松机","馆陶县飞翔机械装备制造有限公司","翻转浅耕深松机","1SLF-225","深松部件个数:5个;深松铲结构型式:凿铲式:是 ;铲间距:450mm","深松部件左5，右5个铲;外形尺寸(长×宽×高):4390×2210×1820mm、配套功率:132.4-154.4kW、铲间距:450mm、深松深度:350-450mm、深松铲结构形式:凿式","冀2018T—169","1700元","1700.00","2022-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求；承诺书错误\r\n","","","","",""]
[32,"耕整地机械","耕地机械","深松机","4-5铲凿铲式深松机","隆尧瑞泰专用设备有限公司","深松浅耕机","1SL-200","深松部件个数:5个;深松铲结构型式:凿铲式:是 ;铲间距:400mm","结构型式：悬挂式          深松部件间距：400mm       深松部件数量：5个       浅耕部件（犁体）数量：6个\n浅耕部件（犁体）幅宽：300mm        犁壁类型：栅条式","T202113130146","1700元","1700.00","2026-05-23","19000.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[33,"耕整地机械","耕地机械","深松机","6铲及以上凿铲式深松机","馆陶县飞翔机械装备制造有限公司","深松机","1S-350","深松部件个数:7个;深松铲结构型式:凿铲式:是 ;铲间距:560mm","深松部件7铲；外形尺寸(长×宽×高):2450×3050×1300MM、结构质量:380KG、配套动力:80.9-88.3KW、工作幅宽:3500MM、铲间距:560MM、深松深度:250-350MM","冀2018T—280（续）","2500元","2500.00","2022-12-31","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[34,"种植施肥机械","播种机械","穴播机","4-5行穴播机","正阳县富田农机设备有限公司","花生施肥精量播种机","2BHSF-4","播种行数:4行","2BHS-4配置参数：结构形式：机械式+悬挂式，配套动力范围：18.7~22.1KW，整机外形尺寸：1920x1750x950，行距：28-32，工作行数：4行，排种器形式：仓转式，排肥器形式：外槽轮式，播种部分传动方式：链条传动。","T202041410109","1000元","1000.00","2025-06-29","0.00","","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[35,"种植施肥机械","播种机械","免耕播种机","4-5行免耕精量播种机","霸州市科维可农业机械有限公司","气力式精密免耕播种机","2BQJM-4","播种行数:4行;排种器型式:精量排种器 ","型号名称\n/\n2BQJM-4型气力式精密免耕播种机\n结构型式\n/\n气力式；牵引式\n配套动力范围\nkW\n40.4～66.2\n工作状态外形尺寸(长×宽×高)\n/\n3000mm×3290mm×1500mm\n作业速度范围\nkm/h\n8～10\n作业小时生产率\nhm²/h\n2.24～2.8\n行距\nmm\n500～700\n工作行数\n行\n4\n工作幅宽\nmm\n2000～2800\n排种器型式\n/\n气力式/金属材料\n排种器数量\n个\n4\n排种器驱动方式\n/\n地轮驱动\n排肥器型式\n/\n外槽轮式\n排肥器数量\n个\n4（使用）+2（备用）\n排肥器驱动方式\n/\n地轮驱动\n种/肥箱容积\n/\n种：30L×4；肥：188L×2\n种/肥箱排量调节方式\n/\n种：链轮调节 ； 肥：手柄调节外槽轮长度\n传动机构型式\n/\n地轮链传动\n开沟器型式\n/\n种：双圆盘；肥：双圆盘\n开沟器数量\n个\n种：4；肥：4\n开沟器深度调节范围\nmm\n0～150\n地轮型式\n/\n胶轮\n地轮直径\nmm\nΦ780\n地轮高度调节范围\nmm\n0～300\n破茬清垄工作部件型式\n/\n凿形铲\n风机型式\n/\n机械式\n风机叶轮直径\nmm\nΦ400\n覆土器型式\n/\nV型胶轮\n镇压器型式\n/\nV型胶轮\n*鉴定机构：","T202000150927","1400元","1400.00","2025-12-30","96000.00","66.2","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[36,"种植施肥机械","播种机械","免耕播种机","4-5行免耕精量播种机","山东亚沃农业机械有限公司","牵引式免耕施肥播种机","2BQMJF-4","播种行数:4行;排种器型式:精量排种器 ","型号名称：2BQMJF-4型牵引式免耕施肥播种机\n结构型式：气力式、牵引式\n配套动力范围：29.4～154.4kW\n工作状态外形尺寸(长×宽×高)：3700×3860×1700\n作业速度范围：4～8km/h\n作业小时生产率：1.1～2.2hm2/h\n行距：35～70cm（可调）\n工作行数：4行\n工作幅宽：140～280cm（可调）\n排种器型式：气吸式\n排种器数量：4个\n排种器驱动方式：地轮驱动\n排肥器型式：外槽轮式\n排肥器数量：4个\n排肥器驱动方式：地轮驱动\n种/肥箱容积：40L×4/350L×2\n排量调节方式：链轮调节、螺杆调节\n传动机构形式：链传动\n开沟盘型式：双圆盘式（排种器）/单圆盘式（排肥器）\n开沟器数量：4个（排种器）/4个（排肥器）\n开沟器深度调节范围：0～70mm\n地轮型式：人字形橡胶轮\n地轮直径：680mm\n地轮高度调节范围：0～90mm\n破茬清垄工作部件型式：圆盘式 拨草轮\n风机型号名称：Y1B9-684\n风机叶轮直径：400mm\n风机转速：5780r/min\n风机风压：0.6MPa\n覆土器型式：V形橡胶轮\n镇压器型式：V形橡胶轮","部20180925","1400元","1400.00","2022-12-31","108000.00","154.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[37,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","霸州市科维可农业机械有限公司","气力式精密免耕播种机","2BQJM-6","播种行数:6行;排种器型式:精量排种器 ","型号名称\n/\n2BQJM-6型气力式精密免耕播种机\n结构型式\n/\n气力式；牵引式\n配套动力范围\nkW\n51.45～99.2\n工作状态外形尺寸(长×宽×高)\n/\n3000mm×4480mm×1500mm\n作业速度范围\nkm/h\n8～10\n作业小时生产率\nhm²/h\n2.4～3.9\n行距\nmm\n500～650\n工作行数\n行\n6\n工作幅宽\nmm\n3000～3900\n排种器型式\n/\n气力式/金属材料\n排种器数量\n个\n6\n排种器驱动方式\n/\n地轮驱动\n排肥器型式\n/\n外槽轮式\n排肥器数量\n个\n6（使用）+2（备用）\n排肥器驱动方式\n/\n地轮驱动\n种/肥箱容积\n/\n30L×6/250L×2\n种/肥箱排量调节方式\n/\n种：齿轮齿数调节 ；肥：手柄调节外槽轮长度\n传动机构型式\n/\n地轮链传动\n开沟器型式\n/\n播种：双圆盘；施肥：双圆盘\n开沟器数量\n个\n种：6；肥：6\n开沟器深度调节范围\nmm\n0～150\n地轮型式\n/\n胶轮\n地轮直径\nmm\nΦ780\n地轮高度调节范围\nmm\n0～300\n破茬清垄工作部件型式\n/\n凿形铲\n风机型式\n/\n机械式\n风机叶轮直径\nmm\nΦ400\n覆土器型式\n/\nV型胶轮\n镇压器型式\n/\nV型胶轮","T202000150928","3200元","3200.00","2025-12-30","144000.00","99.2","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[38,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","任丘市喜洋洋农业机械有限公司","玉米免耕施肥播种机","2BMYZF-6","播种行数:6行;排种器型式:精量排种器 ","结构形式：机械式、悬挂式；配套动力范围（KW）：44.1~88.2；整机外形尺寸（mm）：1500*3500*1150;作业速度范围（km/h）：3~5；作业小时生产率（hm2/h）:0.6~0.7;行距（mm）：600；工作行数（行）：6；作业幅宽（mm）：3600；排种器型式：指夹式、金属材料；排种器数量(个）：6；排种器驱动方式：地轮驱动；排肥器型式：外槽轮式；排肥器数量（个）：6；排肥器驱动方式：地轮驱动；种/肥箱容积（L）：8*6/100*2；种/肥排量调节方式：种：变速箱/肥：变速箱；传动机构型式：链传动+轴传动；开沟器型式：锄铲式；开沟器数量（个）：种：6、肥：6；开沟器深度调节范围（mm）：0~80；地轮型式：橡胶轮；地轮直径（mm）：380；地轮高度调节范围（mm）：0~80；破茬清垄工作部件型式：开沟器+防缠辊；风机型式；风机叶轮直径(mm);覆土器型式：覆土叉；镇压器型式：地轮；","T202113130263","3200元","3200.00","2026-08-18","15000.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[39,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","山东亚沃农业机械有限公司","牵引式免耕施肥播种机","2BQMJF-12","播种行数:12行;排种器型式:精量排种器 ","1.型号名称：2BQMJF-12牵引式免耕施肥播种机\n2.结构型式：气力式；牵引式\n3.配套动力范围：117.6-169.1kW\n4.整机外形尺寸（长×宽×高）：3700mm×8400mm×1700mm\n5.作业速度范围：4～8km/h\n6.作业小时生产率：1.7～6.7\n7.行距：350～700（可调）\n8.工作行数：12\n9.作业幅宽：4200～8400（可调）\n10.排种器型式：气力式、金属材料\n11.排种器数量：12\n12.排种器驱动方式：地轮驱动\n13.排肥器型式：外槽轮式\n14.排肥器数量：12\n15.排肥器驱动方式：地轮驱动\n16.种/肥箱容积：种：40×12 肥;350×4\n17.种/肥排量调节方式：链轮调节（种）、螺杆调节（肥）\n18.传动机构型式：链传动\n19.开沟器型式：双圆盘式（种）/双圆盘式（肥）\n20.开沟器数量：12（种）+12（肥）\n21.开沟器深度调节范围：0～70（种）/0～70（肥）\n22.地轮型式：橡胶轮\n23.地轮直径：720\n24.地轮高度调节范围：0～200\n25.破茬清垄工作部件型式：拨草轮\n26.风机型式：机械驱动离心式\n27.风机叶轮直径：400\n28.覆土器型式：V型对置橡胶轮\n29.镇压器型式：V型对置橡胶轮","T202000370561","3200元","3200.00","2025-09-29","248000.00","169.1","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[40,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","山东亚沃农业机械有限公司","牵引式免耕施肥播种机","2BQMJF-6","播种行数:6行;排种器型式:精量排种器 ","型号名称：2BQMJF-6型牵引式免耕施肥播种机\n结构型式：气力式、牵引式\n配套动力范围：51.5～154.4kW\n工作状态外形尺寸(长×宽×高)：3700×4600×1700\n作业速度范围：4～8km/h\n作业小时生产率：1.6～3.3hm2/h\n行距：35～70cm（可调）\n工作行数：6行\n工作幅宽：210～420cm（可调）\n排种器型式：气吸式\n排种器数量：6个\n排种器驱动方式：地轮驱动\n排肥器型式：外槽轮式\n排肥器数量：6个\n排肥器驱动方式：地轮驱动\n种/肥箱容积：40×6/350×2\n排量调节方式：链轮调节、螺杆调节\n传动机构形式：链传动\n开沟盘型式：双圆盘式（排种器）/单圆盘式（排肥器）\n开沟器数量：6个（排种器）/6个（排肥器）\n开沟器深度调节范围：0～70mm\n地轮型式：人字形橡胶轮\n地轮直径：680mm\n地轮高度调节范围：0～90mm\n破茬清垄工作部件型式：圆盘式拨草轮\n风机型号名称：Y1B9-684\n风机叶轮直径：400mm\n风机转速：5780r/min\n风机风压：0.06MPa\n覆土器型式：V形橡胶轮\n镇压器型式：V形橡胶轮","部20180926","3200元","3200.00","2022-12-31","138000.00","154.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[41,"种植施肥机械","播种机械","免耕播种机","6行及以上免耕精量播种机","山东亚沃农业机械有限公司","牵引式免耕施肥播种机","2BQMJF-8","播种行数:8行;排种器型式:精量排种器 ","型号名称：2BQMJF-8型牵引式免耕施肥播种机\n结构型式：牵引式；气力式\n配套动力范围：47.8~154.4kW\n外形尺寸（长×宽×高）：3600mm×5600mm×1700mm\n作业速度范围：5~9km/h\n作业小时生产率：2.0~5.0hm2/h\n行距：350mm~700mm（可调）\n工作行数：8行\n作业幅宽：2800mm~5600mm\n排种器型式：气力式，金属材料\n排种器数量：8个\n排种器驱动方式：地轮\n排肥器型式：外槽轮式\n排肥器数量：8个\n排肥器驱动方式：地轮\n种/肥箱容积：种：40L×8   肥：350L×2\n种/肥排量调节方式：链轮调节，螺杆调节\n传动机构型式：链传动\n开沟器型式：施肥开沟器：双圆盘式    排种开沟器：双圆盘式\n开沟器数量：施肥开沟器：8个         排种开沟器：8个\n开沟器深度调节范围：0~70mm\n地轮型式：人字形橡胶轮\n地轮直径：0~150mm\n破茬清垄工作部件型式：拔草轮\n风机型式：离心式\n风机叶轮直径：400mm\n覆土器型式：V型橡胶轮\n镇压器型式：V型橡胶轮","T201900370164","3200元","3200.00","2024-11-28","168000.00","154.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[42,"种植施肥机械","栽植机械","水稻插秧机","4行手扶步进式水稻插秧机","山东红旗机电集团股份有限公司","手扶式水稻插秧机","2ZS-430S","行数:4行;手扶步进式:是 ","型号名称\n/\n2ZS-430S型手扶式水稻插秧机\n结构型式\n/\n手扶式\n配套发动机生产企业\n/\n雅马哈动力机械（江苏）有限公司\n配套发动机型号规格\n/\nMZ175\n配套发动机额定功率（或标定功率）\nkW\n3.3\n配套发动机额定转速（或标定转速）\nr/min\n3600\n整机外形尺寸（长×宽×高）\nmm\n2140×1630×910\n作业速度\nm/s\n0.34～0.77\n作业小时生产率\nhm2/h\n0.10～0.18\n单位作业量燃油消耗量\nkg/hm2\n≤4.8\n工作行数\n行\n4\n行距\nmm\n300\n穴距调节机构型式\n/\n机械式\n穴距调节档位数量\n个\n5\n穴距\nmm\n120、140、160、180、210\n插秧深度\nmm\n7～37\n移距\nmm\n14、20\n取秧深度\nmm\n7～17\n插秧频率（单行）\n穴/分\n97～285\n变速方式\n/\n机械变速\n行走轮结构型式（前、后）\n/\n橡胶轮爪式（前）\n行走轮直径（前、后）\nmm\nΦ660（前）\n平衡机构型式\n/\n机械式\n插植臂型式\n/\n曲柄摇杆式","T202100210779","4500元","4500.00","2026-08-31","0.00","3.3","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求；承诺书错误\r\n","","","","",""]
[43,"种植施肥机械","栽植机械","水稻插秧机","6行及以上手扶步进式水稻插秧机","山东红旗机电集团股份有限公司","手扶式水稻插秧机","2ZS-630S","行数:6行;手扶步进式:是 ","型号名称\n/\n2ZS-630S型手扶式水稻插秧机\n结构型式\n/\n手扶式\n配套发动机生产企业\n/\n雅马哈动力机械（江苏）有限公司\n配套发动机型号规格\n/\nMZ175\n配套发动机额定功率（或标定功率）\nkW\n3.3\n配套发动机额定转速（或标定转速）\nr/min\n3600\n整机外形尺寸（长×宽×高）\nmm\n2370×1930×910\n作业速度\nm/s\n0.28～0.77\n作业小时生产率\nhm2/h\n0.10～0.25\n单位作业量燃油消耗量\nkg/hm2\n≤5.6\n工作行数\n行\n6\n行距\nmm\n300\n穴距调节机构型式\n/\n机械式\n穴距调节档位数量\n个\n5\n穴距\nmm\n120、140、160、180、210\n插秧深度\nmm\n7～37\n移距\nmm\n14、20\n取秧深度\nmm\n7～17\n插秧频率（单行）\n穴/分\n80～285\n变速方式\n/\n机械变速\n行走轮结构型式（前、后）\n/\n橡胶轮爪式（前）\n行走轮直径（前、后）\nmm\nΦ660（前）\n平衡机构型式\n/\n机械式\n插植臂型式\n/\n曲柄摇杆式","T202100210780","5700元","5700.00","2026-08-31","0.00","3.3","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书错误\r\n","","","","",""]
[44,"田间管理机械","植保机械","喷杆喷雾机","4-12m悬挂式喷杆喷雾机","台州斯迈特机械有限公司","喷杆式喷雾机","S500-8型喷杆式喷雾机","药箱容积:450L;喷杆长度:7.25m;型式:悬挂式:是 ","结构形式：悬挂式 、工作压力：0.3-0.5MPa 、喷杆长度：7.25m 、喷幅：7.75米、隔膜泵压力：2.0-3.0MPa、额定流量：60-80（L/min）、药箱容量：450L","2018281401000022","730元","730.00","2023-06-24","0.00","","购机补贴(通用类)","浙江省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[45,"田间管理机械","植保机械","喷杆喷雾机","18m及以上悬挂式喷杆喷雾机","新疆天诚农机具制造有限公司","喷杆式喷雾机","3WPX-1200A型悬挂式喷杆喷雾机","药箱容积:1200L;喷杆长度:21m;型式:悬挂式:是 ","整机产品品目：喷杆喷雾机整机。整机结构型式：悬挂式。整机工作压力：0.3-0.5MPa整机外形尺寸：4400×3720×2300mm整机喷杆长度：21000mm限压安全装置：有。喷杆折叠型式：液压折叠。升降型式：液压。驾驶室型式：无。液（气）泵电机泵结构型式：隔膜泵。液泵/电机泵额定压力：2.5MPa。药箱生产方式：采购。限压安全装置结构型式：弹簧式。限压安全装置限定压力：≤0.6MPa。限压安全装置生产方式：采购。喷杆材质：金属管。喷杆生产方式：采购。承压软管材质：橡胶。承压软管允许最大工作压力：3.6MPa。承压软管生产方式：采购，开关组合生产方式：采购。液泵/电机泵额定流量：215L/min液泵/电机泵生产方式：采购。药箱容积：1200.药箱材质：聚乙烯。","2018041401000057","4400元","4400.00","2023-11-21","0.00","","购机补贴(通用类)","新疆生产建设兵团","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[46,"田间管理机械","植保机械","喷杆喷雾机","18m及以上牵引式喷杆喷雾机","新疆天诚农机具制造有限公司","喷杆式喷雾机","3WPQ-4000A型牵引式喷杆喷雾机","药箱容积:4000L;喷杆长度:21m;型式:牵引式:是 ","整机产品品目：喷杆喷雾机。整机结构型式：牵引式。整机工作压力：0.3-0.5MPa整机外形尺寸：6100*3000*3400mm整机喷杆长度：21000mm限压安全装置：有。喷杆折叠型式：液压折叠。升降型式：液压。驾驶室型式：无。液（气）泵电机泵结构型式：隔膜泵。液泵/电机泵额定压力：3.0MPa。药箱生产方式：采购。限压安全装置结构型式：弹簧式。限压安全装置限定压力：≤0.6MPa。限压安全装置生产方式：采购。喷杆材质：金属管。喷杆生产方式：采购。承压软管材质：橡胶。承压软管允许最大工作压力：3.6MPa。承压软管生产方式：采购，开关组合生产方式：采购。液泵/电机泵额定流量：215L/min液泵/电机泵生产方式：采购。药箱容积：4000.药箱材质：聚乙烯。","2018041401000057","4400元","4400.00","2023-11-21","0.00","","购机补贴(通用类)","新疆生产建设兵团","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[47,"田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式四轮转向喷杆喷雾机","青州欧尚农业科技有限公司","喷杆式喷雾机","3WPZ-400A型自走式喷杆喷雾机","功率:19.72马力;药箱容积:400L;离地间隙:0.89m;喷杆长度:8.5m;型式:自走式:是 ;四轮驱动;四轮转向:是 ","整机产品品目：喷杆喷雾机；结构形式:自走式。外形尺寸: 2900×2100×2300 ;工作压力: 0.5-0.8 ;驱动型式:四轮驱动;转向型式:四轮转向;整机限压安全装置：有；喷杆长度: 8500mm ;喷杆折叠型式:手动折叠;喷杆升降型式:手动升降;离地间隙: 890mm ;驾驶室型式:无;轴距: 1550mm ;前后最大轮距: 1340mm ;前/后轮外径: 800mm ;前/后轮胎宽: 40mm ;轮胎型式:实心橡胶轮胎;限压安全装置结构型式:弹簧式,限定压力:≤0.96 ;配套动力名称:汽油机;结构型式:双缸风冷四冲程;功率: 14.5/3600/r/min ;液泵结构型式:三缸柱塞泵;额定压力: 1.5～2.5;额定流量: 14～22L/min ;药箱材质:塑料;药箱容积: 400L ;喷杆材质:塑料;最高允许工作压力: 1 .2MPa ;承压管材质：塑料；蓄电池类型:免维护铅酸蓄电池;容量: 50Ah;","2018281401000067","13400元","13400.00","2023-12-12","45000.00","14.5","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[48,"田间管理机械","植保机械","喷杆喷雾机","18-50马力自走式四轮转向喷杆喷雾机","潍坊爱地植保机械有限公司","自走式喷杆喷雾机","3WP-700","功率:22.3马力;药箱容积:700L;离地间隙:1.1m;喷杆长度:10m;型式:自走式:是 ;四轮驱动;四轮转向:是 ","功率：16.4KW；发动机型号：3C100LWS-C1 ；发动机生产厂商：大同工业株式会社；排放标准：国三；型式：自走式；四轮驱动、四轮转向；药箱容量：700L；离地间隙：1.1m；","T201937370106","13400元","13400.00","2024-10-24","68000.00","16.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[49,"收获机械","谷物收获机械","自走履带式谷物联合收割机（全喂入）","4kg/s及以上自走履带式谷物联合收割机（全喂入）","浙江柳林农业机械股份有限公司","全喂入联合收割机","4LZ-4.0A1","全喂入:是 ;喂入量:4kg/s;自走型式:自走履带式 ","结构型式：全喂入履带自走式；整机外形尺寸 (长×宽×高)mm：5260×2850×2680；整机质量kg：2900；割台工作幅宽mm：2100；履带节距×节数×宽度：90 mm× 50 节×400 mm；履带轨距mm：1100。","T201900340832","26700元","26700.00","2024-12-30","138000.00","65","购机补贴(通用类)","浙江省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[50,"收获机械","谷物收获机械","自走履带式谷物联合收割机（全喂入）","4kg/s及以上自走履带式谷物联合收割机（全喂入）","浙江柳林农业机械股份有限公司","全喂入联合收割机","4LZ-4.0B1","全喂入:是 ;喂入量:4kg/s;自走型式:自走履带式 ","结构型式：全喂入履带自走式；整机外形尺寸 (长×宽×高)mm：5100×2500×2650；整机质量kg：3280；割台工作幅宽mm：2100；履带节距×节数×宽度：90 mm× 50 节×450 mm；履带轨距mm：1100。","T201900340820","26700元","26700.00","2024-12-30","148000.00","70","购机补贴(通用类)","浙江省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[51,"收获机械","玉米收获机械","自走式玉米收获机","4行摘穗剥皮型自走式玉米收获机","凤城市鑫钢机械制造有限公司","自走式玉米收获机","4YZ-4D","收获行数:4行;工作幅宽:2.5m;型式:自走式(摘穗剥皮型):是 ","型号名称：4YZ-4D型自走式玉米收获机；结构形式：轮式+摘穗+剥皮；配套发动机型号：YN4EZ080-30CR;配套发动机生产企业：昆明云内动力股份有限公司；配套发动机结构形式：直列、立式、水冷、四冲程、自然吸气、高压共轨；配套发动机功率：58.8kW;配套发动机额定转速：2400r/min;整机外形尺寸（长×宽×高）：6380×2520×3350；工作行数（通道数）：4行；行距：580mm；工作幅宽：2500mm；最小离地间隙：250mm；作业速度：1.0-4.5km/h;作业小时生产率：0.13-0.4h㎡/h;单位面积燃油消耗量：≤23kg/h㎡；果穗升运器布置位置：右置；果穗升运器结构形式：刮板+链条；摘穗机构形式：立式摘穗辊；摘穗辊/板数量：8个；剥皮机构形式：橡胶辊；剥皮棍数量：12个；割台型式：卧式；割刀型式：往复式切割器；脱粒滚筒数量：0个；主脱粒滚筒型式：无；主脱粒滚筒尺寸（外径×长度）mm：无；风扇数量：1个；风扇型式：离心式；风扇直径：475mm；凹板筛型式：无；清选筛型式：无；卸粮方式：液压翻转；秸秆粉碎还田机构型式：无；驾驶室型式：普通式；变速机构型式：（4+1）×2机械式；驱动型式：四驱；驱动方式（前/后）：机械驱动/机械驱动；制动器型式（前/后）；鼓式/鼓式；轴距：2300mm；导向轮轮距：1600mm；驱动轮轮距：1650mm；导向轮轮胎规格：9.5-16；驱动轮轮胎规格：9.5-16；履带节距：无；打（压）捆机构数量：无。","T20212121070","53500元","53500.00","2026-10-10","0.00","58.8","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[52,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.154m2及以上方捆捡拾压捆机","弗驰瑞特（青岛）农业机械有限公司","方草捆打捆机","9YFQ-1.8","捡拾宽度:1.8m;打结器数量:2个;方捆:是 ;压缩室截面积(宽×高):0.1656m²","型号:9YFQ-1.8\n捡拾器宽度:1800mm\n捡拾器结构形式:弹齿式\n压缩室截面尺寸(宽×高):460mm×360mm\n打结器类型:D 型\n打结器数量:2个\n工作状态外形尺寸(长×宽×高):6110mm×2880mm×1600mm\n非固定式配套动力:≥36.8KW\n执行标准：GB/T 25423-2010","部20190452","16300元","16300.00","2023-12-31","140000.00","0","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[53,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.154m2及以上方捆捡拾压捆机","弗驰瑞特（青岛）农业机械有限公司","方草捆打捆机","9YFQ-1.9","捡拾宽度:1.95m;打结器数量:2个;方捆:是 ;压缩室截面积(宽×高):0.2m²","型号:9YFQ-1.9\n捡拾器宽度:1950mm\n捡拾器结构形式:弹齿式\n压缩室截面尺寸(宽×高):500mm×400mm\n打结器类型:D 型\n打结器数量:2个\n工作状态外形尺寸(长×宽×高):6700mm×3120mm×1700mm\n非固定式配套动力:≥50KW\n执行标准：GB/T 25423-2010","部20190451","16300元","16300.00","2023-12-31","160000.00","0","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[54,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.162m2及以上方捆捡拾压捆机","郎宝全","方草捆打捆机","9YF-2.3","捡拾宽度:2.3m;打结器数量:2个;方捆:是 ;压缩室截面积(宽×高):0.1656m²","型号名称/9YF-2.3方草捆打捆机  挂接方式/牵引式    捡拾宽度mm2300    喂入口宽度mm/    捡拾器结构型式/弹齿式     喂入器结构型式/拨叉喂入机构    打结器型式/D型    打结器数量个2    压缩室截面尺寸（宽×高）mm460×360    配套动力范围kW35～60    配套发动机（电动机）额定功率kW/    配套发动机（电动机）额定转速r/min/   捆扎方式/自动绳打捆","T202023230137","16300元","16300.00","2025-10-11","128000.00","35","购机补贴(通用类)","黑龙江","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[55,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.162m2及以上方捆捡拾压捆机","山东常林派克农业机械有限公司","秸秆饲料捡拾打捆机","9YFQ-2.2","捡拾宽度:2.2m;打结器数量:/个;方捆:是 ;压缩室截面积(宽×高):0.1638m²","型号名称：9YFQ-2.2型秸秆饲料捡拾打捆机；挂接方式：牵引式；捡拾程度：2200mm；捡拾器结构型式：锤爪式；喂入器结构形式：螺旋连续喂入机构；捆扎方式：自动网打捆；压缩室截面尺寸（宽*高）：360X455；配套动力范围：88-120kw;","T202142420239","16300元","16300.00","2026-04-29","190000.00","100","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：承诺书不符合要求\r\n","","","","",""]
[56,"收获机械","饲料作物收获机械","打（压）捆机","压缩室截面积（宽×高）0.162m2及以上方捆捡拾压捆机","襄阳祥盛农业机械有限公司","方草捆打捆机","9YFQ-2.2","捡拾宽度:2.2m;打结器数量:2个;方捆:是 ;压缩室截面积(宽×高):0.162m²","型号名称：9YFQ-2.2型方草捆打捆机；挂接方式：牵引式；捡拾宽度：2230mm；捡拾器结构型式：拨叉喂入机构；打结器型式：D型；打结器数量：2个；压缩室截面尺寸：440*365mm","鄂2019233","16300元","16300.00","2024-07-17","54300.00","0","购机补贴(通用类)","湖北省","评阅不通过","专家：不通过","专家：投档技术参数：不符合填报要求。\r\n","","","","",""]
[57,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1m及以上圆捆捡拾压捆机","黑龙江农垦畜牧工程技术装备有限公司","圆捆捡拾切碎压捆机","9YK-1250","捡拾宽度:1.95m;圆捆:是 ;压缩室直径:/m;压缩室宽度:/m","捡拾器宽度:1950mm 捡拾器结构型式:弹齿式 卷压滚筒转速:180r/min 卷压滚筒数量:2个 工作状态外型尺寸（长*宽*高）:4100mm*2460mm*2465mm 配套动力:88kW","黑2018064","16300元","16300.00","2022-12-31","460000.00","","购机补贴(通用类)","黑龙江","评阅不通过","专家：不通过","专家：投档技术参数：不符合填报要求。\r\n","","","","",""]
[58,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1m及以上圆捆捡拾压捆机","黑龙江农垦畜牧工程技术装备有限公司","圆捆捡拾切碎压捆机","9YK-1600","捡拾宽度:1.95m;圆捆:是 ;压缩室直径:/m;压缩室宽度:/m","捡拾器宽度:1950mm 捡拾器结构型式:弹齿式 卷压滚筒转速:180r/min 卷压滚筒数量:2个 工作状态外型尺寸（长×宽×高）:4000mm*2550mm*2600mm 配套动力:88kW","黑2018065","16300元","16300.00","2022-12-31","488000.00","","购机补贴(通用类)","黑龙江","评阅不通过","专家：不通过","专家：投档技术参数：不符合填报要求。\r\n","","","","",""]
[59,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1m及以上圆捆捡拾压捆机","呼伦贝尔市华迪牧业机械有限公司","卷捆圆打捆机","9YA-1.5","捡拾宽度:1.9m;圆捆:是 ;压缩室直径:1.2m;压缩室宽度:1.5m","捡拾器宽度：1900mm；卷压滚筒转速：115r/min；卷压滚筒数量：14个；工作状态外形尺寸（长×宽×高）：4200mm×2880mm×2300mm；配套动力：≥60kw;圆捆机压缩室直径：1200mm,压缩室宽度：1500mm。","T201915150031","16300元","16300.00","2024-12-30","0.00","","购机补贴(通用类)","内蒙古自治区","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。承诺书过期\r\n","","","","",""]
[60,"收获机械","饲料作物收获机械","打（压）捆机","压缩室直径1.2m及以上圆捆捡拾压捆机","呼伦贝尔市华迪牧业机械有限公司","卷捆圆打捆机","9YA-2.2","捡拾宽度:2.2m;圆捆:是 ;压缩室直径:1.2m;压缩室宽度:1.4m","捡拾器宽度：2200mm；卷压滚筒转速：115r/min；卷压滚筒数量：14个；工作状态外形尺寸(mm):4400mmX3000mmX2210mm；配套动力：≥80kw；圆捆机压缩室直径：1200mm,压缩室宽度：1400mm。","部20170075","23700元","23700.00","2021-12-31","0.00","","购机补贴(通用类)","内蒙古自治区","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。承诺书过期。\r\n","","","","",""]
[61,"收获机械","茎秆收集处理机械","秸秆粉碎还田机","1.5-2m秸秆粉碎还田机","石家庄金牛农机制造有限公司","秸秆收集机","4JS-165","作业幅宽:1.65m","作业幅宽:1.65m；收集器型式：甩刀式","T202013130428","1600元","1600.00","2025-12-29","15000.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：详细配置参数：不符合填报要求。\r\n","","","","",""]
[62,"收获机械","茎秆收集处理机械","秸秆粉碎还田机","2-2.5m秸秆粉碎还田机","石家庄市中州机械制造有限公司","秸秆切碎还田机","1JQ-230","作业幅宽:2.3m","结构形式：侧边皮带传动，配套动力：73.5～80.9kw,纯工作小时生产率：0.7～1.0hm2/h,外形尺寸（长×宽×高）：1330×2600×1100，结构质量：630Kg，工作幅宽：2.30m，最小离地间距：390≥300，作业前进速度：3.3～5km/h，切碎轴转速：2200r/min，切碎机结构最大回转半径：R260mm，切碎机构总安装刀数：76把。","T202013130380","1800元","1800.00","2025-12-29","0.00","","购机补贴(通用类)","河北省","评阅不通过","专家：不通过","专家：承诺书过期\r\n","","","","",""]
[63,"收获后处理机械","干燥机械","谷物烘干机","批处理量4-10t循环式谷物烘干机","安徽省久泰农业装备有限公司","批式循环谷物干燥机","5HJT-4.5","批处理量:4.5t;循环式:是 ","拨粮轮电机0.2kw；提升机电机1.5kw；排湿风机4kw。","2017TJ422","14700元","14700.00","2021-12-31","0.00","6.8","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[64,"收获后处理机械","干燥机械","谷物烘干机","批处理量4-10t循环式谷物烘干机","安徽省久泰农业装备有限公司","批式循环谷物干燥机","5HJT-5","批处理量:5t;循环式:是 ","拨粮轮电机0.2kw；提升机电机0.75kw；排湿风机4kw。","2019TJ028","14700元","14700.00","2023-12-31","0.00","4.95","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。承诺书不符合要求\r\n","","","","",""]
[65,"收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-15B","批处理量:15t;循环式:是 ","型号规格：5HXH-15B\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n2082×1855×9746mm\n批次处理量：15t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1220个/mm\n装机容量：27.73m3\n缓苏段高度：7320mm","2019TJ370","22600元","22600.00","2023-12-31","108000.00","9.02","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[66,"收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","安徽省久泰农业装备有限公司","批式循环谷物干燥机","5HJT-12","批处理量:12t;循环式:是 ","拨粮轮电机0.2kw；提升机电机0.75kw；排湿风机4kw。","2019TJ029","22600元","22600.00","2023-12-31","0.00","4.95","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。承诺书不符合要求\r\n","","","","",""]
[67,"收获后处理机械","干燥机械","谷物烘干机","批处理量10-20t循环式谷物烘干机","宁波天海制冷设备有限公司","热泵型谷物干燥机","5HXRG-100","批处理量:10t;循环式:是 ","型号名称：5HXRG-100型热泵型谷物干燥机\n结构型式：循环式；\n干燥方式：间接加热；\n烘干机机体外形尺寸（长*宽*高）（mm）：2060*1650*7450；\n批次处理量（t）:10;\n干燥速率(%/h):0.4~1.0;\n干燥段高度（mm）:920(数量1段)；\n缓苏段高度（mm）:5520(数量1段)；\n有效容积（m3）:18.2;\n热风温度范围（℃）：35~60；\n排粮电机功率（kw）：0.1；\n提升机生产率（t/h）:10;\n提升机电机功率（kw）：1.5；\n热风机数量：1；\n热风机型号名称：4-72-6A型离心式通风机；\n热风机转速（r/min）:1450;\n热风机风压（Pa）:1139-724;\n热风机流量(m3/h):6677-13353\n热风机电机功率（kw）:4;\n烘干机电机总功率（kw）：7.07；\n热泵型号名称：5RWF80型热泵型干燥热风机\n热泵额定功率（输入功率）（kw）：30.2；\n热泵额定制热量（输出热量）（KJ/h）:396000;\n热泵压缩机型式：涡旋式；\n热泵压缩机数量（个或组）：6；\n热泵辅助电加热功率（kw）:13.5;\n热泵输出热风最高温度（℃）：60.","T201900320769","22600元","22600.00","2024-12-30","180000.00","7.07","购机补贴(通用类)","浙江宁波","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[68,"收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-20B","批处理量:20t;循环式:是 ","型号规格：5HXH-20B\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n2275×2275×9955mm\n批次处理量：20t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1240个/mm\n装机容量：37.29m3\n缓苏段高度：7320mm","2019TJ371","26300元","26300.00","2023-12-31","0.00","11.97","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，\r\n承诺书不符合要求","","","","",""]
[69,"收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-20C","批处理量:20t;循环式:是 ","型号规格：5HXH-20C\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n2279×2279×11704mm\n批次处理量：20t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1240个/mm\n装机容量：36.12m3\n缓苏段高度：7320mm","2019TJ246","26300元","26300.00","2023-12-31","148000.00","8.47","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[70,"收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-22C","批处理量:22t;循环式:是 ","型号规格：5HXH-22C\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n2779×2279×11279mm\n批次处理量：22t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1240个/mm\n装机容量：39.9m3\n缓苏段高度：6710mm","2019TJ247","26300元","26300.00","2023-12-31","158000.00","8.97","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[71,"收获后处理机械","干燥机械","谷物烘干机","批处理量20-30t循环式谷物烘干机","安徽省久泰农业装备有限公司","批式循环谷物干燥机","5HJT-20","批处理量:20t;循环式:是 ","拨粮轮电机0.2kw；提升机电机1.5kw；排湿风机7.5kw。","2017TJ421","26300元","26300.00","2021-12-31","0.00","11.47","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[72,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30C","批处理量:30t;循环式:是 ","型号规格：5HXH-30C\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n2282×3581×11926mm\n批次处理量：30t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1500个/mm\n装机容量：55.7m3","2019tj372","46900元","16900.00","2023-12-31","230000.00","14.32","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[73,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30D","批处理量:30t;循环式:是 ","型号规格：5HXH-30D\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n(2280×2974×11149)+（1697×1390×600）mm\n批次处理量：30t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1220个/mm\n装机容量：53.78m3","2019TJ248","46900元","46900.00","2023-12-31","200000.00","16.52","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[74,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽森米诺农业科技有限公司","批式循环谷物干燥机","5HXH-30E","批处理量:30t;循环式:是 ","型号规格：5HXH-30E\n干燥方式：间接加热\n干燥机机体外形尺寸(长×宽×高)\n(2280×2974×12556)+（1697×1390×600）mm\n批次处理量：30t\n干燥速率：0.5～1.2%/h\n干燥段数量/高度：1/1220个/mm\n装机容量：55.8m3","2019TJ249","46900元","46900.00","2023-12-31","210000.00","14.32","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，承诺书不符合要求\r\n","","","","",""]
[75,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","安徽省久泰农业装备有限公司","批式循环谷物干燥机","5HJT-30","批处理量:30t;循环式:是 ","拨粮轮电机0.4kw；提升机电机2.2kw；排湿风机5.5kw*2。","2017TJ750","46900元","46900.00","2021-12-31","0.00","14.1","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：不通过，\r\n承诺书不符合要求","","","","",""]
[76,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","滁州奥岚格机械有限公司","批式循环谷物干燥机","5H-30","批处理量:30t;循环式:是 ","外形尺寸(长×宽×高):5000×4890×11570mm,整机质量:5280kg,循环批处理量:30t,处理方式：批式循环，加热方式：间接加热，电机总功率:18kw,箱体尺寸(长×宽×高):3160×2360×9100mm,结构形式：固定式","2017TJ050","46900元","46900.00","2021-12-31","0.00","","购机补贴(通用类)","安徽省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[77,"收获后处理机械","干燥机械","谷物烘干机","批处理量30t及以上循环式谷物烘干机","河南迪普森农业开发有限公司","循环式谷物干燥机","5HGX-30","批处理量:30t;循环式:是 ","烘干机机体外形尺寸（长×宽×高）2904mm×2264mm×11035mm；批处理量：30t；结构型式：循环式；有效容积：54m³；热风温度范围：40℃~120℃；烘干机电机总功率：24.073kW；热风炉热功率：400000kcal/h；热风炉和燃烧器燃料种类：天然气","T202100520842","46900元","45900.00","2026-08-31","198000.00","","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[78,"收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市天诚干燥设备有限公司","粮食烘干机","5HSHN-150","处理量:150t;连续式:是 ","处理量：161.5t/d，连续式\n干燥能力（t.%/h）：100.9\n配套动力（kw）：72.9","黑垦鉴2017045","69000元","69000.00","2021-12-31","0.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求,承诺书过期。\r\n","","","","",""]
[79,"收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市天诚干燥设备有限公司","粮食烘干机","5HSHN-200","处理量:200t;连续式:是 ","处理量：264t/d,连续式\n干燥能力（t.%/h）：164.7\n配套动力（kw）：108.5","T20190606102","69000元","69000.00","2024-12-31","0.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[80,"收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市天诚干燥设备有限公司","粮食烘干机","SFH-300","处理量:300t;连续式:是 ","处理量：384.2t/d,连续式\n干燥能力（t.%/h）：241.7；\n配套动力（kw）：172.5。","黑垦鉴2019026（续）","69000元","69000.00","2023-12-31","0.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：不通过，承诺书过期。\r\n","","","","",""]
[81,"收获后处理机械","干燥机械","谷物烘干机","处理量100t/d及以上连续式谷物烘干机","开原市天诚干燥设备有限公司","粮食烘干机","SFH-500","处理量:500t;连续式:是 ","处理量：528.2t/d,连续式\n干燥能力（t.%/h）：327.9\n配套动力（kw）：272.9","黑垦鉴2019027（续）","69000元","69000.00","2023-12-31","0.00","","购机补贴(通用类)","辽宁省","评阅不通过","专家：不通过","专家：不通过，承诺书过期\r\n","","","","",""]
[82,"畜牧机械","畜产品采集加工机械设备","贮奶（冷藏）罐","20000L及以上贮奶罐","新乡市新东轻工机械有限公司","贮奶罐","9GW-33.5","容量:33500L","罐体有效容积33.5立方米;罐体外形尺寸(mm):长×长轴×短轴10350×2470×2060;内部尺寸:长×长轴×短轴为10150×2270×1860;罐体外部保温层厚度为100mm;选装空气悬架.选装顶部平台护栏样式和后部操作箱样式.选装侧面人孔.选装罐体不带装饰腰带.ABS系统控制器型号: CM2XL-4S/2M;生产厂:广州瑞立科密汽车电子股份有限公司;侧部防护装置材质为铝合金5083,与车架螺栓和焊接连接,后部防护装置材为Q235A,与车架焊接连接,后防护断面尺寸为140mm×60mm,距地高度为490mm.","T202100010704","18800元","18800.00","2026-08-31","70000.00","","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：铭牌图片：不符合填报要求。\r\n","","","","",""]
[83,"动力机械","拖拉机","轮式拖拉机","30-40马力两轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF350-C","功率:35马力;驱动方式:两轮驱动 ","江动485国Ⅲ、风云机罩、前轮500-15后轮9.5-24、机械转向、单速输出, 便携前配重、单层后配重。","T202037370115","6900元","6900.00","2025-07-06","23046.00","25.74","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：可靠性试验报告：不符合填报要求。\r\n检验报告、推广鉴定报告中的可靠性报告编号与实际提供的可靠性报告不符。","","W201609124","机械工业农业机械产品质量检测中心（济南）","W201401140- Ⅱ","山东省农业机械产品质量监督检验站"]
[84,"动力机械","拖拉机","轮式拖拉机","100马力及以上两轮驱动拖拉机","洛阳依顿重工机械有限公司","轮式拖拉机","ET1000","功率:100马力;驱动方式:两轮驱动 ","100马力、功率:73.5KW、二轮驱动、\"东方红\"系列LR4B3ZU23/0735E国三发动机","T202000020736","24100元","24100.00","2025-12-30","90000.00","73.5","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：没有提供最新要求的承诺书。\r\n","","FH11GW0081/1","国家拖拉机质量监督检验中心","2011KSS051","河南省农业机械试验鉴定站"]
[85,"动力机械","拖拉机","轮式拖拉机","40-50马力四轮驱动拖拉机","常州东风农机集团有限公司","轮式拖拉机","DF454-15","功率:45马力;驱动方式:四轮驱动 ","整机型号、名称：DF454-15；四驱；整机外廓尺寸(长×宽×高及部位)：3305×1440×2320 mm安全架；最小使用质量：1450kg;最小使用比质量：43.81kg/kW；发动机与主离合器联接方式：直联式；翻倾防护装置（驾驶室或安全框架）型式：安全框架。","T201932320127","9900元","9900.00","2024-12-30","44000.00","33.1","购机补贴(通用类)","江苏省","评阅不通过","专家：不通过","专家：可靠性试验报告：不符合填报要求。\r\n检验报告、推广鉴定报告中的可可靠性试验报告编号与实际提供的不符。\r\n","","FH20GW1281","国家拖拉机质量监督检验中心","（2019）委检字整机类第0023号"," 盐城市农业机械试验鉴定站"]
[86,"动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","宁波宁奔奔野农业机械有限公司","轮式拖拉机","604-2","功率:60马力;驱动方式:四轮驱动 ","60马力四轮驱动轮式拖拉机；整机外廓尺寸(长×宽×高)：3505x1590x2390（安全架顶端）3505x1590x2620（驾驶室顶端）； 最小使用比质量47.74（安全架）52.26（驾驶室）; 标定功率：44.2kw","T201932320106","12000元","12000.00","2024-12-30","46000.00","44.2","购机补贴(通用类)","浙江省","评阅不通过","专家：不通过","专家：可靠性试验报告：不符合填报要求。说明中无法证明604-2可以使用904的可靠性报告\r\n","","FH19GW1691、FH20GW1151","国家拖拉机质量监督检测中心","（2017）委字整机类第0170100144号","盐城市农业机械试验鉴定站"]
[87,"动力机械","拖拉机","轮式拖拉机","60-70马力四轮驱动拖拉机","浙江中野农机装备有限公司","轮式拖拉机","604-2","功率:60马力;驱动方式:四轮驱动 ","60马力四轮驱动轮式拖拉机；整机外廓尺寸(长×宽×高)：3505x1590x2390（安全架顶端）； 最小使用比质量47.42(kg/kw); 标定功率：44.5kw","T201932320103","12000元","12000.00","2024-12-30","48000.00","44.5","购机补贴(通用类)","浙江省","评阅不通过","专家：不通过","专家：可靠性试验报告：不符合填报要求。未提供604是否可以使用904可靠性报告的说明\r\n","","FH20GW0781","国家拖拉机质量监督检测中心","（2017）委字整机类第0170100142号","盐城市农业机械试验鉴定站"]
[88,"动力机械","拖拉机","轮式拖拉机","70-80马力四轮驱动拖拉机","常州东风农机集团有限公司","轮式拖拉机","DF704-16","功率:70马力;驱动方式:四轮驱动 ;最小使用比质量:38.35kg/kW","驱动轮数：四轮驱动；发动机标定功率（kW）：51.5；发动机与离合器联接方式：直联式","T202132320087","15300元","15300.00","2026-03-29","60000.00","51.5","购机补贴(通用类)","江苏省","评阅不通过","专家：不通过","专家：产品图片：不符合填报要求。\r\n","","SAM2021021","国家拖拉机质量监督检验中心","HBNJ20200678","湖北三智农业机械检测有限公司"]
[89,"动力机械","拖拉机","轮式拖拉机","90-100马力四轮驱动拖拉机","潍坊力信机械制造有限公司","轮式拖拉机","WLX904","功率:90马力;驱动方式:四轮驱动 ;最小使用比质量:41.00kg/kW","外廓尺寸：4100×1870×2760(选装驾驶室：4100×1870×2700)；驱动型式：四轮驱动；功率：66.2kW; 发动机型号及制造商：4C6-90C33,安徽全柴动力股份有限公司；轴距：2070; 最小使用质量：2590（驾驶室：2770）变更为：2714（驾驶室：2770）; 配重：144/360; 档位数：12+12; 变速箱型式：4×3组成式；是否有驾驶室或安全架：有安全架选装驾驶室。","鄂2019405","21500元","21500.00","2024-11-15","87500.00","66.2","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。\r\n","","HB2019FHZ014/HB2019FHZ013","湖北三智农业机械检测有限公司","NJJC20181014","山东宝鼎农业机械检测有限公司"]
[90,"动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","常州东风农机集团有限公司","轮式拖拉机","DF1204","功率:120马力;驱动方式:四轮驱动 ;最小使用比质量:53.9kg/kW","驱动轮数：四轮驱动；发动机标定功率（kW）：88.2；发动机与离合器联接方式：直联式","T202000321082","31900元","31900.00","2025-12-30","150000.00","88.2","购机补贴(通用类)","江苏省","评阅不通过","专家：不通过","专家：推广鉴定报告：不符合填报要求。\r\n","","FH11GW0011"," 国家拖拉机质量监督检验中心","（2008）委 字 01类第115号","江苏省农业机械试验鉴定站"]
[91,"动力机械","拖拉机","轮式拖拉机","120-140马力四轮驱动拖拉机","常州森犇农业机械有限公司","轮式拖拉机","SK1304","功率:130马力;驱动方式:四轮驱动 ;最小使用比质量:43kg/kW","外廓尺寸(长×宽×高)：4266*2075*2845mm；\n轴距或履带接地长：2300mm；\n常用轮距(前轮/后轮)或轨距：1685/1600mm；\n轮距(前轮/后轮)调整方式：辐板有级可调/辐板有级可调；\n最小使用质量：4060KG标准配重(前/后)：250/160；\n档位数(前进/倒退/爬行)：16F/8R/12\n主变速档位数*副变速档位数/其他档位数：4/3/2\n发动机与离合器联接方式：直联；\n起动方式：电启动；\n翻倾防护装置（驾驶室或安全框架）：SK1504.451.001\n前照灯型号：250.48.010/250.48.010Y\n转向系型式：独立油路全液压转向；\n行车制动系型式：人力操纵静液压盘式制动器；\n驻车制动系型式：手柄操纵；\n前驱动桥型式：旱地型；\n离合器型式：单片干式，蝶形弹簧压紧、独立操纵、双作用\n传动系动力输出轴离合器型式：无\n传动系变速箱型式：组成式4*2*（2+1）；\n主变速箱换档方式：齿啮合套换档；\n副变速箱换档方式：齿啮合套换档；\n履轮胎型号(前轮/后轮)：11.2-24/16.9-34,选装12.4-24,16.9-38,12.4-24,13.6-38水田轮","苏农机（2018）第（0511）号","31900元","31900.00","2022-12-31","13800.00","95.6","购机补贴(通用类)","江苏省","评阅不通过","专家：不通过","专家：最小使用比质量小于43kg/kw。","","FH18GW0511","国家拖拉机质量监督检验中心","（2018）委检字整机类第0034号","盐城市农业机械试验鉴定站"]
[92,"动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","常州东风农机集团有限公司","轮式拖拉机","DF1504","功率:150马力;驱动方式:四轮驱动 ;最小使用比质量:47.1kg/kW","驱动轮数：四轮驱动；发动机标定功率（kW）：110.3；发动机与离合器联接方式：直联式","T202034471","38800元","38800.00","2025-12-28","190000.00","110.3","购机补贴(通用类)","江苏省","评阅不通过","专家：不通过","专家：推广鉴定报告：不符合填报要求。\r\n铭牌图片：不符合填报要求，铭牌所示型号与上报型号不符。\r\n",""," FH14GW0121"," 国家拖拉机质量监督检验中心","（2016）委检字整机类第009号","江苏省盐城市农业机械试验鉴定站"]
[93,"动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","洛阳依顿重工机械有限公司","轮式拖拉机","ET1404","功率:140马力;驱动方式:四轮驱动 ;最小使用比质量:47.96kg/kW","140马力、功率:103KW、四轮驱动、\"东方红\"系列LR6M3ZU23/1030E国三发动机","部20171235","38800元","38800.00","2021-12-31","140000.00","103","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：推广鉴定报告：不符合填报要求；\r\n承诺书：不符合要求。","","ET1304,45,002","国家拖拉机质量监督检验中心","WJ2017CKKX018","河南省拖拉机柴油机产品质量监督检验中心"]
[94,"动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","洛阳依顿重工机械有限公司","轮式拖拉机","ET1504","功率:150马力;驱动方式:四轮驱动 ;最小使用比质量:44.78kg/kW","150马力、功率:110.3KW、四轮驱动、\"东方红\"系列LR6M3ZU23/1103E国三发动机","部20171236","38800元","38800.00","2021-12-31","0.00","110.3","购机补贴(通用类)","河南省","评阅不通过","专家：不通过","专家：承诺书：不符合填报要求。\r\n","","ET1304,45,002","国家拖拉机质量监督检验中心","WJ2017CKKX018","河南省拖拉机柴油机产品质量监督检验中心"]
[95,"动力机械","拖拉机","轮式拖拉机","140-160马力四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF1504F","功率:150马力;驱动方式:四轮驱动 ;最小使用比质量:46.78kg/kW","潍柴150国Ⅲ、16F+8R、爬行挡、前轮14.9-26/后轮18.4-38、强压升降，双速输出540/1000、三路阀、驾驶室、新机罩、进口原装LUK离合器、加大塑料油箱、加强型滑动可调后桥、165A电瓶、加强悬挂、前后配重。\n玉柴国Ⅲ、16F+8R、爬行挡、前轮14.9-26/后轮18.4-38、强压升降，双速输出540/1000、三路阀、驾驶室、新机罩、进口原装LUK离合器、加大塑料油箱、加强型滑动可调后桥、165A电瓶、加强悬挂、前后配重。","部20180067","38800元","38800.00","2022-12-31","129592.00","110.3","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：最小使用比质量小于43kg/kw。","","W201606050","机械工业农业机械产品质量检测中心（济南）","NW201710018","山东省农业机械科学研究院产品质量检测中心"]
[96,"动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF1604B","功率:160马力;驱动方式:四轮驱动 ;最小使用比质量:44.6kg/kW","潍柴160国Ⅲ、16F+8R、爬行挡、前轮12.4-24后轮16.9-34、强压升降，双速输出760/1000、拉线双路阀、驾驶室、新机罩、进口14吋离合器、280L加大塑料油箱、加强型滑动可调后桥、165A电瓶、加强悬挂、液压离合、省油开关、前后配重。鉴定报告变更后，驾驶室车型最小使用质量为5260kg，最小使用比质量为44.6kg/kw。","部20190219","45700元","45700.00","2023-12-31","152638.00","118","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。\r\n","","W201606050、W201609125","机械工业农业机械产品质量检测中心（济南）","WJ2018JKKX007","河南省拖拉机柴油机产品质量监督检验中心"]
[97,"动力机械","拖拉机","轮式拖拉机","160-180马力四轮驱动拖拉机","潍坊华夏拖拉机制造有限公司","轮式拖拉机","华夏1604","功率:160马力;驱动方式:四轮驱动 ;最小使用比质量:44.92kg/kW","功率：160马力；驱动型式：四轮驱动；最小使用比质量：44.92","部20180307","45700元","45700.00","2022-12-31","0.00","118","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：可靠性试验报告：不符合填报要求。\r\n","","NW201704109(因技术扩展，新报告编号为NW201908062)","山东省农业机械科学研究院产品质量检测中心","WJ2017IKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
[98,"动力机械","拖拉机","轮式拖拉机","180-200马力四轮驱动拖拉机","山东瑞泽重工有限公司","轮式拖拉机","RZ1804-F","功率:180马力;驱动方式:四轮驱动 ;最小使用比质量:43.7kg/kW","功率：132.4kw  驱动方式：四轮驱动  变更后最小使用比质量：43.7（安全架机型已取消，只保留驾驶室机型）","部20171012","51200元","51200.00","2021-12-31","180000.00","132.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。\r\n","","  NW202102002\t","山东省农业机械科学研究院产品质量检测中心","2016KKX070","河南省拖拉机柴油机产品质量监督检验中心"]
[99,"动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF2104G","功率:210马力;驱动方式:四轮驱动 ;最小使用比质量:43.8kg/kW","潍柴210国Ⅲ、16F+8R同步器换挡、爬行挡、前轮14.9-28后轮18.4-38、双速输出760/850、三路阀、豪华空调驾驶室、加宽新机罩、进口摩擦片离合器、280L加大塑料油箱、加强型滑动可调后桥、加强悬挂、可调方向机、省油开关,前后配重。鉴定报告变更后，最小使用质量为6760kg,最小使用比质量43.8kg/kw。","部20190218","51200元","51200.00","2023-12-31","171008.00","154.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。","","W201606050","机械工业农业机械产品质量检测中心（济南）","WJ2018JKKX014","河南省拖拉机柴油机产品质量监督检验中心"]
[100,"动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","山东时风（集团）有限责任公司","轮式拖拉机","SF2404","功率:240马力;驱动方式:四轮驱动 ;最小使用比质量:43.6kg/kW","洛柴240马力国Ⅲ、前轮14.9-28后轮18.4-38、32+24梭式同步器和啮合套换挡、双速540/1000、液压转向、分置式强压提升器、电液控制前轮驱动和动力输出、爬行档、三路阀、国产悬挂、空调驾驶室、省油开关、后视影像系统、前后配重。鉴定报告变更后，单胎车型最小使用比质量43.6","部20190217","51200元","51200.00","2023-12-31","171008.00","176.5","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。\r\n","","W201606050","机械工业农业机械产品质量检测中心（济南）","WJ2018JKKX013","河南省拖拉机柴油机产品质量监督检验中心"]
[101,"动力机械","拖拉机","轮式拖拉机","200马力及以上四轮驱动拖拉机","特拉克（潍坊）农业装备有限公司","轮式拖拉机","TK2104-C","功率:210马力;驱动方式:四轮驱动 ;最小使用比质量:43.72kg/kW","变更后：更换加大燃油箱，质量增加：137kg；加装加强板，质量增加：32kg；换装加强型壳体，质量增加：61kg；最小使用质量：6750kg；最小使用比质量：43.72kg/kW。功率：210马力，驱动方式：四轮驱动，排放阶段：国三。","T202000231048","51200元","51200.00","2025-12-30","210000.00","154.4","购机补贴(通用类)","山东省","评阅不通过","专家：不通过","专家：自主变更。\r\n","","WJ2019DFH011","河南省拖拉机柴油机产品质量监督检验中心","(2019）委检字整机类第0012号","盐城市农业机械试验鉴定站"]